NAME
	CCM12 - LabView driver for the Cryocon Model 12 temperature monitor
		using the RS232 interface.
		*****Pre-release version for LabView 6.1*****
SYNOPSIS
	VIs have a prefix 'CC12'.

DESCRIPTION
	The Model 12 is a two-channel cryogenic temperature monitor with
	serial (RS-232) and Ethernet remote interfaces. These drivers
	support the serial interface.

CONTACT
	For information or technical support, contact:
		Cryogenic Control Systems, Inc.
		PO Box 7012
		Rancho Santa Fe, CA 92067

		858 756 3900

		techsupport@cryocon.com

FILES
	CCM12.TXT
		this file
	CCM12.llb
		Library of VIs
	CCM12U.llb
		Library of VIs that the end user should not modify directly.

VIs
	[Application]
	CC_Icon_Tree.vi
		A listing of all VIs available in this library.
	
	[Low Level]
	CC Initialize.vi
		Opens the instrument.
	
	CC_Close.vi
		Closes the instrument.

	CC_IO.vi
		Sends an ASCII command and returns the instrument's response.
		Attaches line terminator character to command.

	CC_Read.vi
		Read string from instrument.

	CC_WriteCmd.vi
		Write ASCII command string to instrument. String must include
		terminator character (\n).

	CC_Error.vi
		Generic error handler.

	CC_Error_Handler.vi
		Used by CC_Error to handle error messages and request user
		response.
	
-----------------------------------------------------------------------	-
(c)2004 Cryogenic Control Systems, Inc.